|  |  |
| --- | --- |
|  | **DATE:** Month / Date / Year  **NAME OF THE SPA: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SPA DAILY WATER TEST RECORDS**  ***Time of testing: 30 minutes before pool opens and then every 2 hours or every 4 hours with automatic sensing device until the pool is closed*** | | | | | | | | | | | | |
| **Time of Day** | **½ hr. before opening**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** | **Time**  **am/pm** |
| **Free Available Chlorine/ Total Bromine** |  |  |  |  |  |  |  |  |  |  |  |  |
| **pH**  **(7.2-7.8)** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Alkalinity**  **(80ppm – 120ppm)** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Water clarity** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Water Temperature (Celsius or Fahrenheit)** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Operator’s Initials** |  |  |  |  |  |  |  |  |  |  |  |  |

**\* Spa Free Available Chlorine should be 5-10ppm, Total Bromine 5-10ppm**

|  |  |  |  |
| --- | --- | --- | --- |
| **SPA DAILY RECORDS** | | | |
| **Records of any emergency**: **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Rescue equipment breakdown:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Back washing:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Cleaning, etc.: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** | **NAME OF TEST** | **PARAMETERS** | **OPERATOR’S INITIALS** |
| **Number of Bathers** | Number = |  |
| **Emergency stop button**  **(if applicable)** | Working/  Not working |  |
| **Water Meter readings** |  |  |
| **Chemical added manually** | Type =  Amount = |  |
| **Ground current leakage and deionizing device (if applicable)** | Working/  Not working |  |
| **Spa Tank Drained/Inspected/Refilled** |  |  |
| **Emergency telephone (not mandatory and is recommended)** | Operational/  Not operational |  |
| **ORP reading**  **(if applicable, and recommended)** | **600 to 900 mV** |  |

Last Updated: Dec 2022